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2 Megapixel IP 
180° Panoramic
Dome CAMERA
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Dimension (unit : mm)
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FEATURES

IP Panoramic Bullet Camera for 180° viewing angle
3 sensor (2M) and 4.3mm fixed lens allows to FOV of 180° with resolution of 6MP total.

Patented External Tilt/Rotation device Technology 
External Rotation and Tilting patented wired mechanism makes the installer to adjust the camera viewing angle without opening the dome cover. With 8X zoom module will ease to focus.












Digital zoom with digital pan 
Supports digital zoom with digital pan. Setting preset and preset tour is also available with this digital zoom and pan.

Real-time High Definition Bullet Camera
Using the state of art video compression engine, real time HD video streams of 1080p can be delivered for recording and monitoring.

Dual codec, Simultaneous Multi Streaming
Dual H/W codec enables to transmit max 2 independent streams with different settings for different requirements. Therefore, it is possible to combine seamless remote video monitoring using H.264 and additional MJPEG can be delivered for Mobile devices such as Smart Phone or PDA.

Local SD Card Backup
Some important sequence of still images can be stored in the SDHC memory card. This action can be configured to work with pre-post- alarm event or a given interval.

Day & Night by ICR
For increased sensitivity of image sensor efficiently, a mechanical actuator can shift infrared (IR) Cut filter to disengage from image path automatically in the low light environment.

POE
Built-in Power over Ethernet (IEEE 802.3at) makes installation easier, cheaper and more secure since Power over Ethernet can take advantage of UPS (uninterrupted power supply), which provides back-up power in case of a power failure.

Weather Proof Design 
Due to IP66 environment protection as well as speed bullet camera will serve you all the time regardless of rain, snow and storm.










Specification
	CAMERA

	Image Device 
	1/2.8” 2.4M Sony Sensor  * 3ea

	Resolution
	1920 (H) x 1080 (V) ~360(V)

	Aspect Ratio 
	HD: 16:9(1x zoom)  ~ 16:3 (1/3x zoom)

	Focal Length 
	4.3mm Board Lens * 3ea

	Horizontal angle 
	180 degree (each lens angle is 70 degree))

	MIN. Illumination 
	COLOR : 0.5Lux @ F2.5, 30IRE
B/W : 0.27Lux

	Day & Night 
	Auto / Day / Night (ICR)

	Shutter Speed 
	Auto / Manual

	Focus
	Manual

	AGC 
	Max 41dB 

	White Balance
	Auto / Auto-Ext / Indoor / Outdoor / Manual / Preset

	IR LED 
	N/A

	TDN
	Filter change mechanism

	Other Functions
	3D DNR , 3 Sensor out in 1/3x Scale down,
1 Sensor out in 1x zoom




	GENERAL

	Camera Posture 
	3 Axis (Pan/Tilt/Rotation)
External tilt and rotation adjustment

	Digital In/Out 
	1 Alarm Sensor In / 1 Out 

	Audio In / Out 
	1 Audio In / 1 Out

	Video Out 
	BNC:  VBS 1.0 Vp-p

	Power
	DC 12V 14W,  PoE 12W
POE IEEE 802.3af

	Approvals 
	FCC, CE, IP66, ROHS 

	Housing 
	Weather proof/Vandal Proof Structure 
Color: Cool Gray

	Material 
	Aluminum Die-casting 

	Dimension 
	Net (Ø x H) Ø150 x 144.9(H) mm

	Weight 
	2Kg

	Operating Temp. 
	-10°C ~ 50°C







	NETWORK

	OS 
	Embedded Linux 

	Video Compression 
	Dual Codec,H.264/MJPEG 

	Video Streaming 
	Multi Streaming CBR/VBR
(Controllable frame rate and Bandwidth) 

	Resolution 
	H.264 : 1080P/D1/CIF/QCIF 
MJPEG : 1080P/D1/CIF/QCIF

	Frame Rate 
	Max. 30 /25  fps 
for 1080P/D1/CIF/QCIF 

	Audio Compression
	Two way, G.711 PCM. μ-law 64kbps 8kHz 

	Local Storage 
	SDHC memory card (card is not included)

	Motion detection 
	Notification: FTP, e-mail,
Alarm out, JPEG Recording on SD

	Alarm 
	Pre-Post Alarm 

	Max No. of Clients 
	10

	Protocols
 Support 
	IPv4 
	ONVIF, TCP/IP, UDP/IP, RTP(UDP), 
RTP(TCP), RTSP, NTP, HTTP,HTTPS, SSL,
DNS, DDNS, DHCP, FTP, SMTP, ICMP, 
SNMPv1/v2c/v3(MIB-2) 

	
	IPv6 
	TCP/IP, HTTP, HTTPS, DHCP 

	
	DDNS 
	Proprietary: NET4C  
Public DDNS services Suport:
www.dyndns.com, www.no-ip.com 

	
	Security 
	HTTPS(SSL), 
Digest Authentication(ID/PW)

	OS Supported 
	Windows 7, Vista, XP , 2000 
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