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1. GENERAL FEATURES

- 360x Zoom Control (Optical 30x, Digital 12x)
- 5.7” Bubble dome enclosure
- Endless 360° Pan Rotation  
- Lightning Speed (MAX.360°/sec) & Smooth Manual Speed 
(MIN. 0.05°/sec)
- Ultra Low Vibration due to S-curved acceleration & deceleration.
- Day & Night (ICR) 
- 1024 Preset Positions with Alphanumeric Labels
- 128 Pattern, 128 Scan and 128 Group Functions
- Power-up Action, Parking Action
- Built-in 2 Sensor Inputs and 1 Relay Output
- IP66 environment protection as well as built-in Fan & Heater 
- Vandal-Proof 
(Dome Cover: PC / Housing & Accessories: AL Die-cast)
- Built-in Fan & Heater

2. PTZ FEATURES

Micro-Step Technology 
Due to the Micro-stepping technology, one step angle is divided by 256. Accordingly, high accuracy as well as ultra low sound noise (under 60dB) can be achieved. Micro-stepping technology enables ultra low speed down to 0.05°/s for high zoom operations. 

Vector Driving 
Based on the shortest time and the smallest cost concept, each Pan and Tilt motion is done with simultaneous and harmonious manner by Vector drive technology. 

3. IP FEATURES

Real-time High Definition Speed Dome Camera
Using the state of art video compression engine, real time HD video streams of 1080p and 720p can be delivered for recording and monitoring.

Triple codec, Simultaneous Multi-Streaming 
Triple H/W codec enables to transmit Max 3 independent streams with different settings for different requirements. Therefore, it is possible to combine seamless remote video monitoring using H.264 with simultaneous transmission of high quality MPEG-4 to Network Video Recorder. Also, additional MJPEG can be delivered for Mobile devices such as Smart Phone or PDA.

Local SD Card Backup 
Some important sequence of still images can be stored in the SDHC memory card. This action can be configured to work with pre-post-  alarm event or a given interval.

4. UNIQUE FEATURES

Virtual Joystick on the Image
Virtual Joystick is inspired by real 3-Axis Joystick. You can decide PT direction by right clicking the image and change the zoom in out by scrolling mouse wheel. The PT speeds are proportional to how much you deviate mouse from the center. Using this function, control of PTZ is done in instinctive manner. 

Auto Map Generation
After installing PTZ, make camera to generate the Scenery Map autonomously. It will process and stitch a series of pictures to make one overall Scenery map. Using Scenery map, you can quickly switch one place to another. By drawing a bow on the map, PTZ will move to the center of the box as well as adjust zoom ratio to match the box. 






Specification
	CAMERA

	Image Device 
	1/2.8” 2.0 Mega Pixel CMOS

	Effective Pixels 
	Approx. 2 Mega pixels 

	Aspect Ratio 
	HD: 16:9   SD: 4:3 

	Zoom 
	X30 Optical Zoom / X12 Digital Zoom 

	Focal Length 
	f = 4.6 ~ 138.0 mm,  F1.6 ~ F4.7 

	Horizontal angle 
	59.5°(W) ~2.1 °(T) 

	MIN. Illumination 
	Color: 1.7 Lux @ 50IRE, F1.6
B/W: 0.3 lux @ 50IRE, F1.6 

	Day & Night 
	Auto / Day / Night (ICR) 

	Focus 
	Auto(Near Limit setting)/ 
Semi Auto/ Manual 

	DNR
	Level Adjustment(1~5)

	Shutter Speed 
	1/1 ~ 1/10000 sec (22Steps)

	AGC 
	Auto / MANUAL / MAX Gain Limit

	White Balance 
	AUTO/ATW/Manual/Indoor/Outdoor/One-Push/SodiumVaporLamp(fix/auto)

	BLC
	OFF/WDR/BLC

	Image Stabilization
	On/Off

	Other Functions
	POWER UP ACTION, Parking Action

	PAN / TILT

	Range 
	Pan : 360°(Endless) 

	
	Tilt : 90°

	Pan/Tilt Speed 
	Preset : 360°/ sec 

	
	Manual : 0.05°~360°/sec 
(Zoom Proportional) 

	
	Scan : 1°~ 360°/ sec 

	Preset 
	1024 Presets with Labels 

	Pattern 
	128 Patterns 

	Scan 
	128 Scans

	Group 
	128 Groups (MAX. 20 Entries for Each Group) 

	Privacy Zone
	Spherical Privacy Zone Masking

	GENERAL

	Digital In/Out 
	2 Alarm Sensor In / 1 Out 

	Video Out 
	BNC:  VBS 1.0 Vp-p 

	Power 
	AC 24V  Heater Off : 23W
Heater On : 55W
High-PoE IEEE 802.3at(40W)

	Approvals 
	FCC, CE, IK10, ROHS, IP66

	Housing 
	Vandal Proof Structure / Color: Cool Gray

	Material 
	Body: Aluminum Die-casting
Clear Bubble: Polycarbonate 

	Dimension 
	Net (H): Ø259 x 265.7 (H) mm 

	Weight 
	Net: 6 Kg, Package: 10.9 Kg 

	Operating Temp. 
	-40°C ~ 50°C / 40°F ~ 122°F 



	NETWORK

	OS 
	Embedded Linux 

	DSP
	TI DM368

	Video Compression 
	Triple Codec,H.264/MPEG4/MJPEG

	Video Streaming 
	Multi Streaming CBR/VBR
(Controllable frame rate and Bandwidth) 

	Resolution 
	H.264 : 1080p/720p/D1/CIF
MJPEG : 1080P/720p/D1/CIF/QCIF
MPEG-4 : 720p/D1/CIF

	Frame Rate 
	Max. 30 fps for 1080p/720p/D1/CIF/QCIF 

	Audio Compression
	Two way, G.711 PCM. μ-law 64kbps 8kHz 

	Local Storage 
	SDHC memory card (Card is not included)

	Motion detection 
	Notification: FTP, e-mail,
Alarm out, JPEG Recording on SD

	Alarm 
	Pre-Pos Alarm 

	Max No. of Clients 
	10

	Protocols
 Support 
	IPv4
	ONVIF, TCP/IP, UDP/IP, RTP(UDP), 
RTSP, NTP, HTTP,HTTPS, SSL,
DNS, DDNS, DHCP, FTP, SMTP, ICMP, 
[bookmark: _GoBack]SNMPv1/v2c/v3(MIB-2) 

	
	IPv6
	TCP/IP, HTTP, HTTPS, DHCP 

	
	DDNS
	Proprietary: NET4C  
Public DDNS services Suport:
www.dyndns.com, www.no-ip.com 

	
	Security
	HTTPS(SSL), 
Digest Authentication(ID/PW)

	OS Supported 
	Windows 7, Vista, XP



<Optional Accessories> 

 (
Ceiling Mount
 (BC04)
) (
Corner Mount (BCO02)
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Pole Mount (BP02)
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SECUBEST Co., Ltd 
145-2, Sangdaewon-dong, Jungwon-gu, Seongnam-si, 
Gyeonggi-do, 462-807, Korea.
Tel: +82-31-781 0147 Fax: +82-31-7773445
E-mail: sales@secubest.com
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